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	SAFETY DATA SHEET


	Dryko™ Asphalt Primer  –  Solvent-Based Bituminous Primer


	HTS Code: 2715.00.0000  |  Revision Date: May 2026  |  Supersedes: January 2026  |  Version: 2.0



	SECTION 1   –   IDENTIFICATION



	Product Name
	Dryko™ Asphalt Primer – Solvent-Based Bituminous Primer

	Trade Name / Brand
	Dryko™ Asphalt Primer

	HTS Code
	2715.00.0000 – Bituminous mixtures based on natural asphalt, bitumen, or mineral tar

	Recommended Use
	Surface primer for asphalt-based membranes, self-adhering sheets, and modified bitumen roofing systems. Promotes adhesion on concrete, masonry, wood, metal, and existing asphalt surfaces.

	Restrictions
	Not for use on EPDM, TPO, PVC, or other synthetic rubber membranes without compatibility testing

	Manufacturer
	Industria Dryko Ltda., Brazil

	US Distributor
	BSKR Brands LLC
2040 Palm Bay Rd NE, Unit 6 #161, Palm Bay, FL 32905

	Phone
	(321) 285-9908

	Email / Website
	info@bskrbrands.com  |  www.bskrbrands.com

	Emergency Contact
	CHEMTREC: 1-800-424-9300 (24-hour)



	SECTION 2   –   HAZARD IDENTIFICATION



	GHS Signal Word: WARNING  |  Flammable Liquid Cat. 3  |  Skin/Eye Irritant



Signal Word: WARNING
GHS Pictograms: Flame (GHS02), Exclamation Mark (GHS07)

Hazard Statements:
1. H226 – Flammable liquid and vapour (Flash point 38°C – 60°C range)
1. H315 – Causes skin irritation
1. H319 – Causes serious eye irritation
1. H336 – May cause drowsiness or dizziness (solvent vapours)

Precautionary Statements:
1. P210 – Keep away from heat, sparks, open flames, and hot surfaces. No smoking.
1. P261 – Avoid breathing vapours.
1. P271 – Use only outdoors or in well-ventilated areas.
1. P280 – Wear protective gloves, eye protection, and face protection.
1. P303+P361+P353 – If on skin or hair: remove/take off all contaminated clothing, rinse skin with water.
1. P501 – Dispose of contents and container in accordance with local regulations.

	SECTION 3   –   COMPOSITION / INFORMATION ON INGREDIENTS



	Component
	CAS Number
	% by Weight

	Oxidized (Blown) Asphalt
	8052-42-4
	45 – 65%

	Aliphatic Petroleum Solvent (Naphtha)
	64742-89-8
	25 – 40%

	Aromatic Solvent / Modifier
	Mixture
	5 – 15%

	Polymer Additive (SBS/APP)
	Mixture
	2 – 8%



	SECTION 4   –   FIRST AID MEASURES



	Eye Contact
	Flush immediately with clean water for at least 15 minutes, lifting eyelids. Seek medical attention if irritation persists.

	Skin Contact
	Remove contaminated clothing. Wash with soap and water. If irritation persists, seek medical advice.

	Inhalation
	Move to fresh air immediately. If breathing is difficult, administer oxygen. Seek medical attention if symptoms persist.

	Ingestion
	Do not induce vomiting. Rinse mouth with water. Seek immediate medical attention.

	Notes to Physician
	Treat symptomatically. Aspiration hazard if vomiting occurs. Monitor for CNS depression from solvent exposure.



	SECTION 5   –   FIRE FIGHTING MEASURES



	Flash Point
	38°C – 60°C (100°F – 140°F) – Flammable liquid (ASTM D93 / ASTM D56)

	Suitable Extinguishing Media
	CO₂, dry chemical powder, foam. Water fog acceptable for cooling only.

	Unsuitable Media
	Direct water stream (causes spattering of burning asphalt)

	Hazardous Combustion Products
	CO, CO₂, acrid hydrocarbon smoke, sulphur dioxide

	Protective Equipment
	Self-contained breathing apparatus (SCBA) and full protective gear. Keep upwind.

	Special Hazards
	Vapours are heavier than air and may travel to ignition sources. Solvent content makes this product flammable. Store away from all ignition sources.



	SECTION 6   –   ACCIDENTAL RELEASE MEASURES



Personal Precautions: Eliminate ignition sources. Wear gloves, eye protection, and respiratory protection. Ensure adequate ventilation.
Environmental Precautions: Prevent entry into drains, waterways, and soil. Notify authorities if large spill reaches a watercourse.
Containment & Clean-Up: Absorb with inert material (sand, earth, vermiculite). Collect in labelled, closable containers. Dispose per Section 13. Do not flush to sewer.

	SECTION 7   –   HANDLING AND STORAGE



Handling:
1. Use only in well-ventilated areas or outdoors; avoid confined spaces
1. Keep away from open flames, sparks, and hot surfaces – NO SMOKING
1. Wear chemical-resistant gloves, safety glasses, and appropriate respiratory protection
1. Avoid prolonged skin contact and inhalation of vapours
1. Allow adequate drying/flash-off time before applying membrane (typically 15–60 min depending on conditions)

Storage:
1. Store in original sealed containers in a cool, dry, well-ventilated area
1. Recommended storage temperature: 5°C – 35°C (40°F – 95°F)
1. Shelf life: 12 months from date of manufacture in unopened containers
1. Keep away from oxidising agents, heat, and ignition sources
1. Keep containers tightly closed when not in use

	SECTION 8   –   EXPOSURE CONTROLS / PERSONAL PROTECTIVE EQUIPMENT



	Engineering Controls
	Use local exhaust ventilation in enclosed or confined spaces. General dilution ventilation required indoors.

	Respiratory Protection
	NIOSH-approved half-face respirator with organic vapour cartridges (OV/P100) when used indoors or in low-ventilation conditions.

	Eye / Face Protection
	Safety glasses or chemical splash goggles.

	Skin / Hand Protection
	Chemical-resistant gloves (nitrile, neoprene, or equivalent). Replace immediately if contaminated.

	OSHA PEL (Naphtha)
	100 ppm TWA (8-hour)

	ACGIH TLV (Naphtha)
	300 ppm TWA (8-hour)

	Asphalt Fume (NIOSH REL)
	0.1 mg/m³ ceiling (15-min)



	SECTION 9   –   PHYSICAL AND CHEMICAL PROPERTIES



	Appearance: Black liquid / semi-liquid
	Physical State: Liquid

	Odor: Strong solvent / asphalt
	Color: Black to dark brown

	Flash Point: 38°C – 60°C
	Boiling Range: 150°C – 200°C (solvent fraction)

	Solids Content: Approx. 55–75% by weight
	Viscosity: 500–2000 cP at 25°C

	Specific Gravity: Approx. 0.85–0.95 g/cm³
	Vapour Pressure: ≤1.5 kPa at 20°C

	Solubility in Water: Negligible / immiscible
	Flammability Class: Flammable Liquid (Class II – NFPA 30)

	VOC Content: Refer to product technical data sheet
	pH: Not applicable



	SECTION 10   –   STABILITY AND REACTIVITY



	Reactivity
	Not reactive under normal conditions of use and storage

	Chemical Stability
	Stable in sealed containers at recommended storage temperatures

	Conditions to Avoid
	Elevated temperatures, open flames, sparks, direct sunlight on containers

	Incompatible Materials
	Strong oxidising agents; avoid contact with strong acids, bases, and chlorinated solvents

	Hazardous Decomposition
	CO, CO₂, hydrocarbons, sulphur compounds – only under combustion or extreme heating

	Hazardous Polymerisation
	Will not occur



	SECTION 11   –   TOXICOLOGICAL INFORMATION



	Acute Toxicity (Oral)
	Low acute oral toxicity expected based on components

	Acute Toxicity (Dermal)
	Low; prolonged contact may cause skin defatting and irritation

	Acute Toxicity (Inhalation)
	Vapours and mists may cause dizziness, headache, and CNS depression at elevated concentrations

	Skin Irritation
	Classified as irritant (H315); repeated exposure may cause dermatitis

	Eye Irritation
	Classified as irritant (H319); may cause temporary redness and discomfort

	Sensitization
	Not expected to be a skin or respiratory sensitizer

	Carcinogenicity
	Oxidised asphalt (IARC Group 3 – not classifiable). Petroleum naphthas not listed as carcinogens (NTP/OSHA). Use adequate ventilation to minimise vapour exposure.

	Reproductive Toxicity
	No data indicating reproductive toxicity under normal use

	STOT (Single Exposure)
	H336 – may cause drowsiness or dizziness from solvent vapours

	STOT (Repeated Exposure)
	Prolonged high-level solvent exposure may affect the CNS; use PPE and ventilation



	SECTION 12   –   ECOLOGICAL INFORMATION



	Aquatic Toxicity
	Petroleum-based solvents are toxic to aquatic organisms; prevent product from entering waterways

	Persistence
	Asphalt components are persistent; petroleum solvents are biodegradable to varying degrees

	Bioaccumulation
	Not expected to bioaccumulate significantly in the environment

	Soil Mobility
	Low mobility in soil; asphalt components adsorb strongly to soil particles

	Other Adverse Effects
	Prevent spills and run-off from reaching waterways, storm drains, or soil



	SECTION 13   –   DISPOSAL CONSIDERATIONS



Dispose of waste material, residue, and empty containers in accordance with all applicable local, state, and federal regulations (40 CFR Parts 261–268). Do not pour down drains or into watercourses. Liquid waste may be classified as flammable / hazardous waste – contact your local waste management authority for guidance. Empty containers may retain residue and should be handled as hazardous waste until properly cleaned.

	SECTION 14   –   TRANSPORT INFORMATION



	DOT (USA)
	Combustible Liquid, NA1993, Flammable Liquids, N.O.S. (Asphalt, Petroleum Naphtha), PG III

	IATA
	Flammable Liquid, UN1993, Flammable liquids, N.O.S., 3, PG III

	IMDG
	Flammable Liquid, UN1993, Flammable liquids, N.O.S., Class 3, PG III, Marine Pollutant: No

	UN Number
	UN1993 (if flash point < 60°C) or NA1993 (DOT Combustible, >60°C) – confirm by product batch flash point

	Packing Group
	III

	Special Precautions
	Keep containers upright and secured. Store separately from oxidisers and foodstuffs during transport.



	SECTION 15   –   REGULATORY INFORMATION



	OSHA HCS (29 CFR 1910.1200)
	This product IS classified as hazardous. SDS required.

	TSCA (15 U.S.C. §2601)
	All components are listed on the TSCA Chemical Substance Inventory or are exempt

	CERCLA / SARA Title III
	Petroleum naphtha components may be subject to SARA Section 313 reporting requirements

	California Prop 65
	Contains petroleum-derived compounds. May contain trace amounts of benzene, a Prop 65 listed chemical. Ensure adequate ventilation.

	HTS Code
	2715.00.0000 – Bituminous mixtures based on natural asphalt, bitumen, or mineral tar



	SECTION 16   –   OTHER INFORMATION



	Revision Date
	May 2026

	Previous Revision
	January 2026

	Version
	2.0

	Prepared By
	BSKR Brands LLC – Regulatory & Compliance Department

	Contact
	info@bskrbrands.com  |  www.bskrbrands.com  |  (321) 285-9908



Key Abbreviations: OSHA – Occupational Safety & Health Administration; GHS – Globally Harmonised System; SDS – Safety Data Sheet; TSCA – Toxic Substances Control Act; CERCLA – Comprehensive Environmental Response, Compensation, and Liability Act; SARA – Superfund Amendments and Reauthorization Act; DOT – Department of Transportation; IATA – International Air Transport Association; IMDG – International Maritime Dangerous Goods; RCRA – Resource Conservation and Recovery Act; IARC – International Agency for Research on Cancer; VOC – Volatile Organic Compound; PPE – Personal Protective Equipment; STOT – Specific Target Organ Toxicity; SCBA – Self-Contained Breathing Apparatus; CNS – Central Nervous System; TWA – Time-Weighted Average; PEL – Permissible Exposure Limit; TLV – Threshold Limit Value; REL – Recommended Exposure Limit.

	DISCLAIMER: The information in this Safety Data Sheet is believed accurate as of the revision date and is provided in good faith without warranty, express or implied. BSKR Brands LLC and Industria Dryko Ltda. assume no liability for injury, loss, or damage arising from use of this product other than as directed. Users are responsible for determining suitability for their specific application and for complying with all applicable regulations.
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