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	☀
	Temperature Range for Application



Apply Dryko™ Seal only when ambient and surface temperatures are within the range below. Applying outside these limits reduces adhesion and may compromise the waterproof seal.

	Recommended Application Temp.
	40°F (4°C) to 120°F (49°C)

	Service Temp. After Install
	-40°F to 180°F (-40°C to 82°C)

	Cold Weather Note
	Store rolls at room temperature before use; cold rolls are stiff and harder to press flat

	Hot Weather Note
	In direct sun, shade the roll and work surface before application to prevent premature tack-off



★  Never apply over frost, ice, or standing water. Check weather forecast — no rain for at least 24 hours after installation.

	1
	Safety First



1. Work on a dry day with no rain in the forecast
1. Wear gloves, safety glasses, and non-slip shoes
1. Use a roof harness
1. Keep out of reach of children

	2
	Inspect and Prepare the Area



1. Remove loose shingles, debris, and damaged material
1. Surface must be dry and structurally sound

	3
	Clean the Surface



1. Brush off dust, granules, and moisture
1. Wipe with a clean cloth if needed
1. Let area fully dry before priming

	4
	Apply Asphalt Primer (When Necessary)



1. Use a brush or roller
1. Apply primer 2–4 inches beyond the hole on all sides
1. Coat both exposed decking and surrounding shingles
1. Allow primer to flash off until tacky (usually 10–20 minutes)

★  Primer ensures proper adhesion and long-term seal

	5
	Cut the Membrane Patch



1. Cut aluminum-coated membrane large enough to overlap the hole
1. Minimum overlap: 4–6 inches on all sides
1. For larger holes, use a 36-inch wide roll for full coverage

	6
	Apply the Aluminum-Coated Asphalt Membrane



1. Center the membrane over the hole
1. Press down starting from the center outward
1. Ensure aluminum side faces up

	7
	Seal and Press



1. Firmly press membrane edges by hand or with a roller
1. Remove air bubbles and wrinkles
1. Make sure edges are fully bonded to shingles

	8
	Final Inspection



1. Confirm full adhesion
1. No exposed decking
1. No lifted edges or gaps

★  Roof is now watertight, UV-protected, and sealed
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