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	☀
	Temperature Range for Application



Apply Dryko™ Seal Primer only when ambient and surface temperatures are within the range below. Applying outside these limits reduces adhesion and may compromise the waterproof seal.

	Recommended Application Temp.
	50°F (10°C) to 104°F (40°C)

	Relative Humidity
	Below 85%

	Cold Weather Note
	Do not apply below 50°F (10°C); product will not flash off properly and adhesion will be compromised

	Hot Weather Note
	Warmer temperatures accelerate drying; work efficiently to avoid premature tack-off



★  Never apply over frost, ice, or standing water. Check weather forecast — no rain for at least 24 hours after installation.

	⚠
	Safety First (Read Before Use)



1. Work on a dry day with no rain in the forecast
1. Wear gloves, safety glasses, and non-slip shoes
1. Use proper fall protection (roof harness) when working at height
1. Avoid skin and eye contact
1. Keep out of reach of children
1. Use in a well-ventilated area

	1
	Inspect the Area



1. Identify damaged or leaking section
1. Ensure surface is structurally sound
1. Fix major damage before applying primer

	2
	Clean the Surface



1. Remove dirt, dust, loose granules, and old sealant
1. Brush thoroughly
1. Wipe with clean cloth if needed
1. Surface must be completely dry

	3
	Apply Primer



1. Use a brush or roller
1. Apply an even coat
1. Extend 2–4 inches beyond repair area
1. Cover exposed decking and surrounding shingles

	4
	Let It Set



1. Allow primer to flash off until tacky
1. Do NOT apply membrane while primer is wet

	5
	Ready for Membrane



1. Once tacky, apply aluminum membrane
1. Adhesion will be significantly stronger

★  Primer ensures proper adhesion and long-term seal

	★
	Pro Tips & Common Mistakes



	Pro Tips
1. Apply only on dry surfaces
1. Do not over-apply
1. Warmer temperatures = faster drying
1. Use on concrete, metal, wood, and porous surfaces
	Common Mistakes to Avoid
1. Applying on wet surfaces
1. Skipping surface cleaning
1. Applying membrane before primer is tacky
1. Using too much primer



	✓
	Performance Benefits



	⬆ Adhesion
Strength
	🛡 Enhanced
Waterproof Seal
	⏳ Extended
Repair Life
	✔ Long-Term
Durability



	↪
	Quick Summary



	1  CLEAN
	2  PRIME
	3  WAIT
	4  APPLY
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